**A picture containing text, sign

Description automatically generated**

**CAMEO**

**Architecture for Manipulating Earth Observation Data**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**D3.1**

**WORK PACKAGE: WP3 Data Quality Assurance**

**DELIVERABLE: 3.1 Data Quality Measures**

**SUBMISSION DATE: 03 05 2023**

**NATURE: WORK PACKAGE OUTPUT REPORT (INTERMEDIATE)**

|  |  |
| --- | --- |
| **Document Control** | |
| **Creator** | **Punit Gupta** |
| **Description** | **The intended design of the Earth Observation Intelligent Data Analytics Services for CAMEO project, as part of deliverable 3.1** |
| **Publisher** | **University College Dublin** |
| **Audience** | **CAMEO Project** |
| **Status** | **Draft** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Version** | **Issue date** | Stage | Changes | Contributor |
| 0.1 | 17/02/2023 | Draft | No previous document | P Gupta |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

**PROJECT IDENTIFICATION**

**Subject: Report on design of the Earth Observation Intelligent Data Analytics Services**

**Domain:**

**REF.:**

**Activity No.**

**ITEM NO.:**

**CONTRACT NO:**

**PRIME CONTRACTOR: University College Dublin**

**EXTERNAL SUPPLIER:**

**COPYRIGHT: University College Dublin**

**Contents**

[1](#_heading=h.gjdgxs) Introduction 4

[1.1](#_heading=h.30j0zll) Purpose of this document 4

[1.2](#_heading=h.1fob9te) Definitions, acronyms, and abbreviations 4

[1.3](#_heading=h.3znysh7) Reference Documents 4

[2](#_heading=h.2et92p0) Intelligent Data Analytics Services 5

[2.1](#_heading=h.tyjcwt) Introduction 5

[2.2](#_heading=h.3dy6vkm) What are the benefits of implementing an IDAS for CAMEO? 5

[2.3](#_heading=h.1t3h5sf) What steps are involved in implementing an IDAS for CAMEO? 6

[3. Data Analytics for CAMEO 7](#_heading=h.4d34og8)

[3.1](#_heading=h.2s8eyo1) Types of Data Analytics 7

[3.2](#_heading=h.17dp8vu) Data Analytics in Earth Observation 7

[3.3](#_heading=h.3rdcrjn) Data Analytics Techniques 9

[3.4](#_heading=h.26in1rg) Data Analytics Toolkits/Packages 9

[3.5](#_heading=h.lnxbz9) Identifying appropriate Data Analytics Services 10

[3.5.1](#_heading=h.35nkun2) Data Analytics Services backlog 11

[4. Conclusion 13](#_heading=h.1ksv4uv)

# 1 Introduction

## 1.1 Purpose of this document

This document describes the intended design of the Earth Observation Intelligent Data Analytics Services for CAMEO project, as part of deliverable 3.1.

It aims to provide:

* Introduction to data quality.
* Identification of various earth observatory sources
* Categorization of earth observatory data types
* Identifying the need for Data Quality and its evaluation matrix
* Design of Data Quality Adjudication Framework

## Introduction to spatial data quality

Understanding spatial data quality is important in Geographic Information Science (GIS) applications. Spatial data are used in a variety of critical applications, including urban planning, environmental management, emergency response, and natural resource management where the accuracy and precision of spatial data can have a significant impact on the decision making, especially when used with predictive analysis. A review of the importance of spatial data quality in GIS data is necessary to understand the factors that affect the quality of spatial data and strategies used to interrogate and maintain spatial data quality. While there is no standard definition for spatial data quality, typically the term refers to the accuracy, completeness, consistency, and currency of the data. One of the key factors that affect spatial data quality is the data acquisition phase. The accuracy of spatial data can be compromised due to errors introduced during data collection, such as measurement errors or errors in data processing of raw data. Therefore, it is essential to ensure that data collection procedures are well-designed and accurately executed to minimise such errors. In this work a review on various applications of spatial data quality is GIS to provide a generalized Spatial Data Quality (SDQ) benchmark to reduce error in spatial data across various domains

Data quality plays an important role in any form of data analysis and predictive analysis. Over the years big data environments like cloud computing, geographic information (satellite images and other earth observatory data) and healthcare have attracted researchers as data were seen as the new oil. These fields have huge scope and findings that can be disclosed using data analysis but data quality plays an important role to conclude a strong finding, or else it may result in error-prone analysis and predictions.

In the field of earth observation, the data are generated by various agencies using different tools and techniques. This can result in an error or incomplete data . Such incomplete data or low-quality data used for analysis may result in low accuracy or even misleading results . Data quality in Geographic Information Science (GIS) is important because accurate and reliable data is essential for making effective decisions. Poor data quality can lead to incorrect conclusions and poor decision-making. In GIS, data quality refers to the degree to which the data meets the requirements for its intended use. This includes factors such as accuracy, precision, completeness, and consistency. To ensure data quality in GIS, it is important to use high-quality data sources, properly maintain and manage the data, and regularly verify and validate the data to ensure it is accurate and up to date. Additionally, proper documentation and metadata are essential for understanding the quality of the data and for ensuring that it is being used correctly.

GIS data primarily consists of raster and vector data types. Both types of data sources and databases suffer from different types of data quality issues and can be assessed with different metrics. In the raster data type the database mostly suffers from the satellite image quality and the quality of data in the image source may be due to resolution, visibility, or noise.

# Motivation

Currently, a huge amount of satellite data is available from various sources varying from low to high resolution with various bands for vegetation and many other applications like ocean data, precipitation time series data, soil temperature data, object accuracy in vector layer. But the issue that exists in the current scenario is to evaluate and find a suitable dataset from existing satellites data (Sentinel 1 -7 and Landsat 1-9 and other GIS vector data like, time series data, Census and other surveys . With such a huge volume of data it becomes difficult to identify useful data for a user defined application with a specific objective. Even when suitable data are sourced, the data an have errors or low data quality [42]. In such cases there is a need of a quality metadata and quality check to be attached to the datasets to make filtration and identification of datasets easier for specific use cases. In this work our aim is to identify existing spatial data quality measures which can be generalized to check for data quality. The data quality metrics may vary from application to application as discussed in section 3. So, this work aims to identify common SDQ parameters for multiple applications.

To understand the importance of data quality in GIS for industry a survey was conducted where industry partners (2) shared their knowledge on data quality. The results are shown in Table 1.

# Table 1: Impact and Importance of Data Quality (Note: Where higher value refers to a high correlation in their use case/application)

|  |  |  |
| --- | --- | --- |
| **SME name** | **A** | **B** |
| Data Quality has a large impact on achieving my goals | 2 | 1 |
| Data Quality is an issue with the datasets that I use | 2 | 2 |
| My workflow has robust processes to assess data quality | 1 | 3 |
| My workflow has robust processes to handle Data Quality issues | 1 | 2 |
| Please rank the following data quality metric based on importance to your typical tasks. [Completeness] | 6 | 2 |
| Please rank the following data quality metric based on importance to your typical tasks. [Semantic Accuracy] | 7 | 6 |
| Please rank the following data quality metric based on importance to your typical tasks. [Lineage / Traceability] | 3 | 7 |
| Please rank the following data quality metric based on importance to your typical tasks. [Temporal Accuracy] | 4 | 4 |
| Please rank the following data quality metric based on importance to your typical tasks. [Positional Accuracy] | 5 | 3 |
| Please rank the following data quality metric based on importance to your typical tasks. [Logical Consistency] | 2 | 5 |
| Please rank the following data quality metric based on importance to your typical tasks. [Attribute Accuracy] | 1 | 1 |

Chart, bar chart

Description automatically generated

Figure 3: Importance of Data Quality Measures for EO SMEs (Note: Where higher value refers to a high correlation in their use case/application)

Figure 3 shows that the data used by the EO SMEs in the survey primarily suffers from semantic accuracy, completeness, positional and temporal accuracy. The EO SMEs were asked how they handle data quality in their workflow. The results are presented in the table below (Table 2).

# Table 2: EO SMEs practices for handling data quality issues.

|  |  |  |
| --- | --- | --- |
| **SME** | **A** | **B** |
| Please indicate any external sources for data validation. (e.g. EPA) | Met Eireann, EPA, ESA, NASA, OpenWeatherMap, Windy.com, EUMETSAT | DAERA, DAFM |
| Please indicate how you currently validate data in your organisation. Please be specific in relation to different data/information products. | Pixel values in satellite images can be validated using in-situ buoys, although this is not always done. Validation work generally occurs as part of R&D / scientific projects. Imagery from providers such as ESA & NASA is generally considered accurate enough for operational purposes. | In-person inspection of agricultural fields, visual inspections of multispectral imagery |
| Please list the current data sources that you use for Ground Truthing. Please indicate if they are proprietary to your company. | We use our in-situ buoys & sensors. Our buoy platforms, data ingress software, and satellite processing chains are proprietary. | Rapid field visit results from agricultural entities. |
| Please indicate how you currently handle outliers or noise in the datasets that you use | For satellite images: land and clouds are masked from the images (not required for marine EO). For in-situ data: outliers are removed if they cannot be explained following investigation. | Outliers are removed from training data past a certain threshold for error. These are visually inspected or validated with in-person ground checks |
| Please indicate any processes that you use to improve data quality when it is found to be poor. | Noise can be mitigated in SAR images using speckle filters (Lee filters etc.). Noise in optical images can be mitigated using smoothing filters, de-striping algorithms, and masking. | Data smoothing, gaussian filters. |
| If you use Landsat data, please indicate if you typically use Collection 1 or Collection 2 | Collection 2 | Collection 2 |

The survey contributed to showcase the data quality issues and practices (Table 2) that exist in the real world and has influenced the design of the proposed data quality modules and frameworks for CAMEO.

# 3 Survey

In this field many studies are being performed by various researchers to define the need and how data quality can be defined for earth observation data.

There exists various types of GIS data and use cases where different data quality metrics plays an important role. In general, GIS data can be divided into raster and vector data types as shown in figure 1, where raster data includes satellite images from various products like MODIS, Landsat, sentinel among others. On the other hand, vector data are various layers added to a map which are generated through the machine-like road maps, river maps, location of hospitals and many more location-based information. This also includes data from various GIS survey and time series data. Both type of data suffer data Quality issues and result in poor analysis. In this section we introduce various quality indexes in raster and vector with some of the related work in that domain.

Graphical user interface, text, application, chat or text message

Description automatically generated

Figure 1. Types of GIS data

Spatial data quality can be evaluated under four different categories which are as follows as shown in figure 2:

1. Precision

2. Consistency

3. Completeness

4. Accuracy

These four SDQ can be used to evaluate data quality where every category does not fits every data type. For raster data precision, completeness and accuracy are main parameters on the other hand for vector data precision, consistency and completeness plays and important role.

Diagram

Description automatically generated

**Figure 2. Classification of Spatial Data Quality (SDQ).**

Graphical user interface

Description automatically generated

**Figure 3. Spatial Data Quality (SDQ) in GIS Raster Data.**

Graphical user interface, application

Description automatically generated

**Figure 4. Spatial Data Quality in GIS Vector Data**

Figure 3 and Figure 4 show the SDQ parameters for raster and vector data respectively. The next sections describe these SDQ metrics in more detail.

3.1. Precision

For raster data precision is evaluated as the image accuracy and the metadata quality which includes bands and other data like depth and number of bands . Data Quality in satellite images refers to the quality of the image and accuracy of the image in relation to the position and size of the object in the image. Several of the GIS products suffer image quality due to low visibility or image resolution.

3.1.1. Accuracy of bands in GIS data

Albanai et.al .[5] showcased a model to evaluate the thermal accuracy of Landsat in the band on the sea surface. This study checks the computational accuracy of satellite images with live data as compared to the vector data available from sea beakers . The work uses bands 10 and 11 from Lansat-8 and compares the accuracy which comes out to be a deviation in accuracy with a mean standard deviation 0.03 over the year. Figure 5 and Figure 6 shows a similar deviation over various seasons for band 10 and 11. The work showcased a deviation in vector data when it was compared with real data from sea beakers.

|  |  |
| --- | --- |
| Chart, bar chart, histogram  Description automatically generated | **Chart, bar chart, histogram  Description automatically generated** |
| **Figure 5 . Mean-variance in band 10 [5]** | **Figure 6 . Mean-variance in band 11 [5]** |

3.2. Completeness

Completeness is defined as the accuracy of the data in the raster image which can be cloud coverage, land cover accuracy where as in vector data it is defined at the percentage of missing data or null values. Where accuracy is defined as the precision of detecting clouds in image with cloud shadow and further classification.

3.2.1. Cloud cover and masking

Ackerman, S [10] has presented a cloud masking algorithm for the MODIS (Moderate Resolution Imaging Spectroradiometer) database. The algorithm uses MODIS and LIDAR data from the Department of Energy (DOE) Atmospheric Radiation Measurement (ARM) Program Southern Great Plains (SGP) site in Lamont. The algorithm is trained to find the cloud mask in the image with high accuracy. It uses 3 years of MODIS data.

Kopp, T [11] has proposed a (Visible Infrared Imager Radiometer Suite) VRIIS model for detecting cloud masks. This model used VCM (visible cloud mask) model. This algorithm is used to classify the various land use like cloud, land, soil, water, coastal & snow. This is a product of the Joint Polar Satellite System program, the algorithm is defined for the MODIS database. The model can define multi-layered clouds, can separate clouds and aerosols and cloud shadows.

Cesar Aybar et.al. [12] has proposed a deep learning model for cloud detection for Sentinel-2. The model is called CloudSEn12 which is defined to detect cloud, cloud shadow and multi-layer clouds. The model is trained on 49400 image data. The main importance of this model as compared to other models is it can differentiate between thick and thin models. The work is also compared with other existing models like Fmask, Sen2Cor and UNetMob. The figure below shows the performance of CloudSEN-12 with various other existing models for cloud and cloud shadow classification.


Chart, histogram

Description automatically generated

**Figure 7. Performance of various cloud detection model [13]**

Segal R M. et.al. [13] have proposed and improved the S-2 cloud mask algorithm using a CNN model. The work provides better accuracy for cloud detection compared to the original S-2 cloud mask. The work uses sentinel-2 data for testing and training the model, with 13 spectral bands and resolution of 10m. the testing was mostly conducted on images from the Fiji island database.

Qiu.S. et.al. [14] in this work has proposed an improved version of the FMASK algorithm for Lansat4, Landsat 8 and sentinel-2 images. This is one of the tools which allows cloud masking for multiple datasets available with high accuracy. This work demonstrates FMASK 4.0, a version of the algorithm integrated with separate models for cloud masking over land and water to maintain high accuracy. Figure 8. shows the working of FMASK 4.0 where various auxiliary data are integrated for training purposes and detection of cloud, cloud shadow, urban detection and snow detection.



**Figure 8 Existing FMASK model workflow [14]**

Additionally, there are various other models which are presented in in Table 1. This FMASK model proposes the feasibility and study of various other ML models that can be used for better performance.

Table1: cloud detection and masking techniques

|  |  |  |
| --- | --- | --- |
| **Reference** | **Model** | **Model used** |
| 15 | SEN12MS-CR-TS | SEN12MS-CR-TS |
| 16 | SECloud Mask | spectral-temporal classifiers |
| 17 | Fmask | fusion of Images and Auxilary data |
| 18 | dsen2-cr | deep residual neural network |
| 19 | DEcloud | Deep learning model |
| 20 | Luojia1-Cloud-Detection | Threshold-based cloud detection |
| 21 | Deep-gaofill | deep convolutional autoencode for cloud detection and gap filling |
| 22 | CloudFCN | Full CNN |
| 23 | Ukiscsmask | convolution neural network |
| 24 | STGAN | cloud removal using Spatiotemporal Generative Models |
| 25 | Cloud-Net | fully convolutional network (FCN) based cloud detection |
| 26 | CloudMattingGAN | GAN |
| 27 | ES-CCGAN | haze removal using cycle generative adversarial network |
| 28 | Cdnet | basic CNN with low dataset and low accuracy |
| 29 | GLNET | CNN based cloud and non cloudy classification |
| 30 | CDNetV2 | CNN based model cloud detection and removal |
| 31 | AISD | deep learning model for shadow detection |
| 32 | Cloud-GAN | Model used deeip learning GAN model |
| 33 | Mec-GAN | https://github.com/andrzejmizera/MEcGANs |
| 34 | CloudXNet | https://github.com/shyamfec/CloudXNet |
| 35 | SEnSEl | https://github.com/aliFrancis/SEnSeI |

[15] presents a new remote sensing model aimed at cloud removal in multitemporal images. The authors start by highlighting the importance of remote sensing data in various applications, including land use and land cover classification, crop yield estimation, and urban planning. However, the presence of clouds in the images can significantly affect the accuracy of these applications. To address this issue, the authors introduce SEN12MS-CR-TS, a new data set that includes multimodal and multitemporal remote sensing data with and without clouds.

In another work a model was proposed to remove the noise from the images and new pixels were generated using geometric median. This authors in [16] propose an API name SECloud Mask to regenerate pixel and fill the noise in the image with high quality pixels where noise can be cloud and cloud shadow.

FMask[15] a tool kit and algorithm aimed to identify cloud, cloud shadow and snow in satellite images. The toolkit was released in 2015 which has been improved over the period with latest release of FMask 4.0. The tool is made for Landsat 4-8 and sentinel 2 satellite images. The model uses Haze Optimized Transformation (HOT) for prediction of cloud and snow in images. The tool is used to define Normalized Difference Snow Index (NDSI) and Normalized Difference Cloud Index (NDCI).

In this generation of artificial intelligence various work are being proposed using deep learning and neural networks. Various trained machine learning models are be produced using deep learning, artificial neural network, CNN, RNN and many more. In [18] a similar work in presented for cloud detection and removal from sentinel-2 images using deep neural network. The work showcases collection of huge satellite data and training the data for cloud detection using deep RNN which is neural network with large number of hidden layers and neurons. The work is useful to detect and remove cloud from image and regenerate the removed pixels using optical representation of near land structure.

Another work using deep CNN [21] resulted in a tool called Deep-gaofill. The tool is an image gap filling model using deep convolutional neural network which is trained for filling the pixels in radar images. This work is just a demo since it is not trained with large dataset.

CloudFCN [22] is a CNN based detection machine learning model for raster images. The model identifies thick clusters of cloud and their shadow over the area. The model is trained with Landsat and sentinel images for training purpose. The work uses RGB band images for training purpose. The work is compared with SVM , PCA and single-pixel neural networks (NNs) [39,40,41]

Similar work for cloud detection using fully convolutional network [23, 25] is proposed and used in tools named Cloud-Net and Ukiscsmask. Ukiscsmask is trained using Landsat OLI dataset over a U-Net CNN model for cloud detection the work is an extension of existing work where this model extends the cloud classification to five classes (“shadow”, “cloud”, “water”, “land” and “snow/ice”). Where prior to this only 3 classes exists (Cloud, land, no cloud).

On the other hand, Cloud-Net [25] is a trained machine learning model using CNN for cloud detection in Landsat 8 data. The model is very specific in nature due to its training data restrictions. The work is compared with existing FMask model for the accuracy of cloud detection. The proposed cloud-Net model proved to provide better accuracy in term of detection of cloud in Landsat 8 data.

Some of the similar proposed ML based toolkit for cloud and cloud shadow detection are Cdnet and GLNET [27,28,29]. These are some simple CNN based model for cloud detection and classification into thick and thin cloud. For cloud shadow detection using deep learning is shown in AISD [31] where deep Deeply Supervised convolutional neural network for Shadow Detection (DSSDNet) is used to improve the cloud shadow detection raster Landsat data. In [32] a Distortion Coding Network method is proposed for cloud detection. In [33] another cloud detection algorithm is proposed using GAN which is an unsupervised model with higher accuracy than any other model but need huge data for training. Similar work using machine learning are proposed in [34,35] for cloud detection for various satellite datasets. Since the accuracy in GIS models depends on the quantity of dataset trained and the variety of datasets, so new developments are taking place to make the model more accurate.

After cloud detection and removal the empty pixels need to be filled/generated, for this some of the work using mathematical modles [16,21] are proposed. In some of new research Machine learning models and deep learning models are used to improve the accuracy and quality of the pixels. For example, in [26] author has proposed a Generative adversarial network to use deep neural network to generate similar pixel for replacing cloud pixels.

This data quality refers to the amount of useful data out of the whole data set. In the case of earth observatory data where various platforms provide satellite images based on AOI (Area of Interest). In such cases a polygon drawn may not provide complete data and so the data completeness quality need to be checked.

Similarly other factors that impact data completeness are cloud cover, haze or fog in the atmosphere. As discussed above various cloud detection and classification algorithms have been proposed including machine learning models. This allows users to know the useful or visible data that can be used for analysis. Similarly, classification algorithms allow you to know the degree of the visible area, partially visible or cloud-covered area.

Data completeness plays an important role in various applications like landcover, forest cover and sea or water bodies. In these specific GIS applications users are interested in knowing the quality of data in terms of useful data for their need like land cover or sea cover without processing the data. In such case data completeness allows you to know the data completeness in terms of land cover and sea cover which allows the user know the data quality without computing the data which allows the user to select the high-quality data for analysis.

3.3. Accuracy

In [1] data quality for watershed data which is a timeseries data is discussed. Mauro et.al. [1] presented a study on the importance of data quality in watershed streamflow and sediment data analysis. The work showcases the study of fine sediment yield in the Goodwin Creek watershed of 21.3 km. The work is a study on the effect of various spatial data, and geomorphology on land use and land cover maps. The work uses various existing models like Soil and Water Assessment Tool (SWAT) and AVSWAT to study the performance. The result shows that GIS data has a significant effect on the models to predict the streamflow and sediment data analysis where the data quality plays an important role to improve the accuracy of the model.

In [42] a study on SDQ for American Community Survey Data 2013 has been performed. This study showcased the data quality errors in the American census data in various parameters like age income where discrepancy in these parameters for some counties was very high using mean and median as data quality parameters.

[2]In this work, the authors have performed a study on the spatial data quality for data from various sources like maps, vector layers and satellite images. The work showcases a mathematical model to study the data quality accuracy parameter from various sources and product databases where each product does not fulfil all data quality parameters.

* + 1. Accuracy of the object in GIS data

Zhan, Q [4] has showcased a study on accuracy in object identification and placement in vector maps. The work showcases the study on the error and changes in accuracy in object detection to find the exact object like streets, buildings, trees and many more. The author has given a model to match the vector data which is a combination of lines and points which allows finding the changes like missing objects or errors in the data. On comparison of different data, the accuracy was found to 81.8%. The study area is in Amsterdam and the Ravensburg site.

Barazzetti et.al. [6] studied the accuracy using RMSE ( Root-Mean-Square Error) of the images between sentinel 2 and Landsat-8 images where the comparison of the image registered at 10m and 15m are taken into consideration. The work also studies the accuracy of various bands B1-B11 using RMS (root-mean-square error). The study showcases that error in various reference bands 4(10m), 5(20m) and 9(60m) where RMS error was recorded in each image which varies from 0.19-0.55. This can also be used to define the correctness of the data. The study was conducted for images of various countries where the RMSE value for each country was evaluated and where a variation in RMSE value of various locations was recorded.

Marangoz, A. M [7] studied the accuracy of land use classification between Sentinel-2 and Landsat-8 images. The work aims to first define the land use classification using Sentinel images and compare the accuracy using RGB and NIR bands. In the second phase, the same process is done with Landsat images to find the land use and classification in the image. The work has showcased the lower accuracy in both sentinel and Landsat data with an accuracy of 0.74 and 0.66 correspondingly for RGB and NIR bands. The work also studies the accuracy of object-based classification where the accuracy of the sentinel and Landsat was recorded to be 80.7% and 73.4%. This showcases that for land use and object-based classification sentinel images have high accuracy than lansat-8.

**Table 2.**

Table

Description automatically generated

Frantz, D. [8] proposed a system called FORCE which is a tool to generate images with high accuracy for land use that combines the images from sentinel, Landsat, NANA and ESA. The tool is designed to take multiple images and fuse them into one to generate a single image and bands which has high-accuracy data. FORCE is a data fusion tool to improve the spatial resolution of land surface images using Landsat and Sentinel ARD.

In [9] Kocaman. S et.al. have studied the image quality and geometric quality of Landsat 7 and 8 where various issues were highlighted in the global database at zoom levels and in the histogram which was further improvised by histogram and other techniques. The work highlights that the data suffer from the colour difference. The study also studies the advantages and disadvantages of the various data sources as shown in Table 3.

**Table 3**.

Table

Description automatically generated

* + 1. Structural Accuracy in GIS data

In this section, some of the work of structural data quality in GIS data and its role is showcased. In [36] the authors demonstrate the use of GIS data to measure the accuracy of a bridge deformation. This refers to the evaluation of degradation of data accuracy which allows you to evaluate any error in a structure like bridges, buildings and high-rise structures. This work uses a ground-based radar system to collect the structural data and then further comparison and evaluation The work was able to evaluate the accuracy of the deformation in bridge.

Similar work was done by the authors in [37] to measure the change in land use spread in urban area using GIS where the accuracy of the data has an important role to play. The accuracy of such data needs to evaluate to measure the consistency in the data collected and the data showcased. This work uses thematic accuracy to evaluate the correctness of the data. In another work [38] Another standard for data positioning in GIS data [38] is National Standard for Spatial Data Accuracy (NSSDA) which is used in the US for positional accuracy of data in GIS data using a normal distribution. Where the normal distribution defines the spread of position error at a specific location.

3.5 Data Quality Summary

Table 4 shows the final summary of the work where the SDQ benchmark can be defined as precision, consistency, completeness and accuracy for any GIS data which can be raster or vector. This benchmark SDQ will allow users to evaluate data, which can be raster or vector. This will allow users to select an appropriate data before moving on to further analysis. These SDQ will also user to select data for analysis based on accuracy, completeness and precision this will allow user to get the required data the application domain that may me land cover, ocean, forest cover or forest fire analysis but on the other hand if the data has low completeness in that case user has large amount of data but less useful data for its application.

**Table 4. Summary of Work on Spatial Data Quality**

|  |  |  |
| --- | --- | --- |
| **Data Quality parameter** | **GIS data quality** | **Related Work** |
| Percission | Image Resolution,  Quality of Bands,  Number of Bands | [3,5-7,13] |
| Consistency | Logical consistency | [1-2] |
| Completeness | Useful Land data, Useful Sea data,  Useful Forest data | [10-33] |
| Accuracy | Structural Accuracy,  Accuracy of bands ,  Accuracy of the object,  Spatial accuracy,  Temporal accuracy,  Thematic accuracy | [4-9] [36-38] |

# 4 Spatial Data Quality Services

## 4.1 Introduction

As the term Spatial data quality is defined in section 1. This module is responsible to take data in the form of raster and vector from the warehouse and evaluate the data quality parameters defined in sections 2 & 3. This will help the user to evaluate whether the raw data is useful for computing and the quality of the information in it. The module will have the capability to evaluate both raster (Image) data and vector data in various forms.

3.6 Design Plan for Spatial Data Quality (SDQ) Service

This section showcases the proposed architecture for data quality module. As s in 2.3, below is a visual representation of how the data quality services will evaluate the different types of GIS datasets from various metrics. Figure 2 showcased the proposed architecture where the architecture has 2 sub-services for raster data and vector data.

* SDQ for Raster Data
  + This service constitutes of four major components. First the extraction of area of interest from the satellite data. The second step is basic image pre-processing to convert the GIS data to image format for computing. The third step to evaluate the data for SDQ using performance parameters from evaluation metrics. The fourth step to score the data for data quality based on the performance metrics in step three.
* SDQ for Vector Data
  + This service is to evaluate the data quality for vector data which can be further used in GIS for machine learning or further analysis. This service will evaluate the SDQ and score the quality of data to help users in deciding the usefulness of its use case. The module allows used upload the tabular/ Vector data and get the score at the end.

Figure 3 shows a demonstration of a prototype SDQ for raster data. The figure shows the working of the SDQ module with Dell warehouse to fetch the data using search API. The SDQ micro service further produces metadata with data quality parameters for raster data. Figure 4 demonstrates the prototype of raster SDQ and its working with existing search API.

Graphical user interface, application


Description automatically generated

*Fig 2: Design of Data Quality Services accessed by CAMEO end-users.*

*Graphical user interface, application

Description automatically generated*

*Fig 3: Demonstration of a prototype of SDQ for raster data*



*Fig 4: Demonstration of a prototype of SDQ to evaluate the useful land. water and green cover.*

# 4. Conclusion

Implementation of SDQ micro-service with CAMEO will provide an evaluation of data quality score for GIS data.

The service will ensure the evaluation of :

* Precision
* Consistency
* Completeness
* Accuracy
* Timeliness

The above giver spatial data quality is evaluated for raster and vector data to evaluate the final score to cluster the data as very low, low, medium and high. This will allow the user to understand whether the GIS data is useful for the use case they want to design.

# References

[1] M. di Luzio, J. G. Arnold, and R. Srinivasan, “Effect of GIS data quality on small watershed stream flow and sediment simulations,” *Hydrol Process*, vol. 19, no. 3, pp. 629–650, Feb. 2005, doi: 10.1002/hyp.5612.

[2] S. Ying, Y. Lei, and J. Zhanming, “Evaluating spatial data quality in GIS database,” *2007 International Conference on Wireless Communications, Networking and Mobile Computing, WiCOM 2007*, pp. 5962–5965, 2007, doi: 10.1109/WICOM.2007.1463.

[3] Trigila, A., Iadanza, C., & Spizzichino, D. (2010). Quality assessment of the Italian Landslide Inventory using GIS processing. *Landslides*, *7*(4), 455-470.

[4] Zhan, Q., Molenaar, M., Tempfli, K., & Shi, W. (2005). Quality assessment for geo‐spatial objects derived from remotely sensed data. *International Journal of Remote Sensing*, *26*(14), 2953-2974.

[5] Albanai, J. A., & Abdelfatah, S. A. (2022). Accuracy assessment for Landsat 8 thermal bands in measuring sea surface temperature over Kuwait and North West Arabian Gulf. *Kuwait Journal of Science*, *49*(1).

[6] Barazzetti, L., Cuca, B., & Previtali, M. (2016, August). Evaluation of registration accuracy between Sentinel-2 and Landsat 8. In *Fourth International Conference on Remote Sensing and Geoinformation of the Environment (RSCy2016)* (Vol. 9688, pp. 71-79). SPIE.

[7] Marangoz, A. M., Sekertekin, A., & Akçin, H. (2017). Analysis of land use land cover classification results derived from sentinel-2 image. *Proceedings of the 17th International Multidisciplinary Scientific GeoConference Surveying Geology and Mining Ecology Management, SGEM*, 25-32.

[8] Frantz, D. (2019). FORCE—Landsat+ Sentinel-2 analysis ready data and beyond. *Remote Sensing*, *11*(9), 1124.

[9] Kocaman, S., Debaecker, V., Bas, S., Saunier, S., Garcia, K., & Just, D. (2020). Investigations on the Global Image Datasets for the Absolute Geometric Quality Assessment of MSG SEVIRI Imagery. The International Archives of Photogrammetry, Remote Sensing and Spatial Information Sciences, 43, 1339-1346. Doi: 10.5194/isprs-archives-XLIII-B3-2020-1339-2020

[10] Ackerman, S. A., Holz, R. E., Frey, R., Eloranta, E. W., Maddux, B. C., & McGill, M. (2008). Cloud detection with MODIS. Part II: validation. Journal of Atmospheric and Oceanic Technology, 25(7), 1073-1086.

[11] Kopp, T. J., Thomas, W., Heidinger, A. K., Botambekov, D., Frey, R. A., Hutchison, K. D., ... & Reed, B. (2014). The VIIRS Cloud Mask: Progress in the first year of S‐NPP toward a common cloud detection scheme. *Journal of Geophysical Research: Atmospheres*, *119*(5), 2441-2456.

[12] Aybar, C., Ysuhuaylas, L., Loja, J., Gonzales, K., Herrera, F., Yali, R., ... & Gómez-Chova, L. (2022). CloudSEN12-a global dataset for semantic understanding of cloud and cloud shadow in Sentinel-2.

[13] Segal-Rozenhaimer, M., Li, A., Das, K., & Chirayath, V. (2020). Cloud detection algorithm for multi-modal satellite imagery using convolutional neural-networks (CNN). *Remote Sensing of Environment*, *237*, 111446.

[14] Qiu, S., Zhu, Z., & He, B. (2019). Fmask 4.0: Improved cloud and cloud shadow detection in Landsats 4–8 and Sentinel-2 imagery. *Remote Sensing of Environment*, *231*, 111205.

[15] Ebel, P., Xu, Y., Schmitt, M., & Zhu, X. X. (2022). SEN12MS-CR-TS: A Remote-Sensing Data Set for Multimodal Multitemporal Cloud Removal. *IEEE Transactions on Geoscience and Remote Sensing*, *60*, 1-14.

[16] Roberts, D., Mueller, N., McIntyre, A. (2017). High-dimensional pixel composites from Earth observation time series. IEEE Transactions on Geoscience and Remote Sensing, PP, 99. pp. 1--11.

[17] Zhu, Z., Wang, S., & Woodcock, C. E. (2015). Improvement and expansion of the Fmask algorithm: Cloud, cloud shadow, and snow detection for Landsats 4–7, 8, and Sentinel 2 images. *Remote sensing of Environment*, *159*, 269-277.

[18] Meraner, A., Ebel, P., Zhu, X. X., & Schmitt, M. (2020). Cloud removal in Sentinel-2 imagery using a deep residual neural network and SAR-optical data fusion. *ISPRS Journal of Photogrammetry and Remote Sensing*, *166*, 333-346.

[19] Cresson, R., Narçon, N., Gaetano, R., Dupuis, A., Tanguy, Y., May, S., & Commandre, B. (2022). Comparison of convolutional neural networks for cloudy optical images reconstruction from single or multitemporal joint SAR and optical images. *arXiv preprint arXiv:2204.00424*.

[20] Ou, J., Liu, X., Liu, P., & Liu, X. (2019). Evaluation of Luojia 1-01 nighttime light imagery for impervious surface detection: A comparison with NPP-VIIRS nighttime light data. *International Journal of Applied Earth Observation and Geoinformation*, *81*, 1-12.

[21] Cresson, R., Ienco, D., Gaetano, R., Ose, K., & Minh, D. H. T. (2019, July). Optical image gap filling using deep convolutional autoencoder from optical and radar images. In *IGARSS 2019-2019 IEEE International Geoscience and Remote Sensing Symposium* (pp. 218-221). IEEE.

[22] Francis, A., Sidiropoulos, P., & Muller, J. P. (2019). CloudFCN: Accurate and robust cloud detection for satellite imagery with deep learning. *Remote Sensing*, *11*(19), 2312.

[23] Wieland, M.; Li, Y.; Martinis, S. Multi-sensor cloud and cloud shadow segmentation with a convolutional neural network. Remote Sensing of Environment, 2019, 230, 1-12.

[24] Uzkent, B. U., Sarukkai, V. S., Jain, A. J., & Ermon, S. E. (2019). Cloud removal in satellite images using spatiotemporal generative networks.

[25] Mohajerani, S., & Saeedi, P. (2019, July). Cloud-Net: An end-to-end cloud detection algorithm for Landsat 8 imagery. In *IGARSS 2019-2019 IEEE International Geoscience and Remote Sensing Symposium* (pp. 1029-1032). IEEE.

[26] Zou, Z., Li, W., Shi, T., Shi, Z., & Ye, J. Generative Adversarial Training for Weakly Supervised Cloud Matting Supplementary Material.

[27] Hu, A., Xie, Z., Xu, Y., Xie, M., Wu, L., & Qiu, Q. (2020). Unsupervised haze removal for high-resolution optical remote-sensing images based on improved generative adversarial networks. *Remote Sensing*, *12*(24), 4162.

[28] Yang, J., Guo, J., Yue, H., Liu, Z., Hu, H., & Li, K. (2019). CDnet: CNN-based cloud detection for remote sensing imagery. *IEEE Transactions on Geoscience and Remote Sensing*, *57*(8), 6195-6211.

[29] Sun, H., Lin, Y., Zou, Q., Song, S., Fang, J., & Yu, H. (2021). Convolutional neural networks based remote sensing scene classification under clear and cloudy environments. In *Proceedings of the IEEE/CVF International Conference on Computer Vision* (pp. 713-720).

[30] Guo, J., Yang, J., Yue, H., Tan, H., Hou, C., & Li, K. (2020). CDnetV2: CNN-based cloud detection for remote sensing imagery with cloud-snow coexistence. *IEEE Transactions on Geoscience and Remote Sensing*, *59*(1), 700-713.

[31] Luo, S., Li, H., & Shen, H. (2020). Deeply supervised convolutional neural network for shadow detection based on a novel aerial shadow imagery dataset. *ISPRS Journal of Photogrammetry and Remote Sensing*, *167*, 443-457.

[32] Zhou, J., Luo, X., Rong, W., & Xu, H. (2022). Cloud Removal for Optical Remote Sensing Imagery Using Distortion Coding Network Combined with Compound Loss Functions. *Remote Sensing*, *14*(14), 3452.

[33] Hasan, C., Horne, R., Mauw, S., & Mizera, A. (2022). Cloud removal from satellite imagery using multispectral edge-filtered conditional generative adversarial networks. *International Journal of Remote Sensing*, *43*(5), 1881-1893.

[34] Kanu, S., Khoja, R., Lal, S., Raghavendra, B. S., & Asha, C. S. (2020). CloudX-net: A robust encoder-decoder architecture for cloud detection from satellite remote sensing images. *Remote Sensing Applications: Society and Environment*, *20*, 100417.

[35] Crisler, M., Essig, R., Estrada, J., Fernandez, G., Tiffenberg, J., Haro, M. S., ... & Sensei Collaboration. (2018). SENSEI: first direct-detection constraints on sub-GeV dark matter from a surface run. *Physical review letters*, *121*(6), 061803.

[36] Erdélyi, J., Kopáčik, A., & Kyrinovič, P. (2020). Spatial data analysis for deformation monitoring of bridge structures. *Applied Sciences*, *10*(23), 8731.

[37] Herold, M., Scepan, J., & Clarke, K. C. (2002). The use of remote sensing and landscape metrics to describe structures and changes in urban land uses. *Environment and planning A*, *34*(8), 1443-1458.

[38] Zandbergen, P. A. (2008). Positional accuracy of spatial data: Non‐normal distributions and a critique of the national standard for spatial data accuracy. *Transactions in GIS*, *12*(1), 103-130.

[39] Li, P., Dong, L., Xiao, H., & Xu, M. (2015). A cloud image detection method based on SVM vector machine. *Neurocomputing*, *169*, 34-42.

[40] Ahmad, A., & Quegan, S. (2012). Cloud masking for remotely sensed data using spectral and principal components analysis. *Engineering, Technology & Applied Science Research*, *2*(3), 221-225.

[41] Hughes, M. J., & Hayes, D. J. (2014). Automated detection of cloud and cloud shadow in single-date Landsat imagery using neural networks and spatial post-processing. *Remote Sensing*, *6*(6), 4907-4926.

[42] Wong, D. W., & Sun, M. (2013). Handling data quality information of survey data in GIS: A case of using the American Community Survey data. *Spatial demography*, *1*, 3-16.